The T-BAR UP fixture by JLC-Tech is specified with either 3" (order code -3-) or 6" (order code -6-) end caps to set its height from the finished ceiling plane. The mounting height of the IES file should be placed at either 3" or 6" below the room height to properly account for the end cap of choice.

For more information contact quotes@jlc-tech.com